{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Select","Sheet1"],"not_rendered":{"charts":0,"images":9,"macros":1,"external_links":0,"defined_names":15,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Select","index":0,"n_rows":25,"n_cols":22,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[null,"Dielectric’s TFU-UT Series turnstile antenna is designed for  broadband omni directional horizontally polarized operation. The TFU-UT features a simple feed system and durable construction.",null,"Dielectric’s DLP Series antenna is designed as an economical single channel choice for low power TV.  ",null,"Dielectric’s TLP Series antenna is designed for single channel, low wind load, horizontal, circular or elliptically polarized operation.  Custom azimuth and elevation patterns available upon request",null,"Dielectric’s TUA-M Series panel antenna is designed for broadband horizontally polarized operation.  The panel is a key building block for antenna system kit. The kit includes ﬂexline jumpers and power dividers.  Custom azimuth and elevation patterns available upon request",null,"Dielectric’s TUM-LP panel antenna is designed for Broadband Elliptical Polarization.  Custom azimuth and elevation patterns available upon request",null,"Dielectric’s TUL panel antenna is a key building block for antennas with different azimuth and elevation patterns.  Custom azimuth and elevation patterns available upon request",null,"Dielectric’s TLS-V Series antenna is designed as a low cost, low windload alternative for the VHF broadcaster. ",null,"Dielectric’s TLSV-BB Series antenna is designed as a broadband, low-cost, low-windload alternative for the high band VHF broadcaster. ",null,"Dielectric’s TLP-BB Series antenna is designed speciﬁcally for multichannel operation with low wind load.",null,"Dielectric’s WB-LP Series antenna is an economical broadband antenna option for the low power market. The WB-LP utilizes the same design as the standard WB.",null,"Dielectric’s WB Series antenna is designed speciﬁcally for wide band multichannel operation with low wind load."]
[null,"Contact Factory",null,"DLP Prop Generator",null,"TLP Prop Generator",null,"Contact Factory",null,"Contact Factory",null,"Contact Factory",null,"TLS-V Prop Generator",null,"Contact Factory",null,"Contact Factory",null,"WB-LP Prop Generator",null,"WB Prop Generator"]
[null,"Broadband 470-608 MHz",null,"One 6MHz channel: 470-692 MHz",null,"One 6MHz channel: 470 - 692 MHz",null,"Broadband  470-692 MHz",null,"Broadband 470-692 MHz",null,"60MHz bandwidth 470-692MHz",null,"One 6MHz channel: 174 to 216MHz",null,"Broadband 174 to 216MHz",null,"Operating range 48 MHz (6 channels) within 470 - 860 MHz",null,"Broadband 470 - 698 MHz",null,"Broadband 470 - 698 MHz"]
[null,"VSWR,  1.2:1 over operating band",null,"VSWR,  1.1:1 over operating band",null,"VSWR,  1.1:1 over operating band",null,"VSWR,  1.1:1 over operating band",null,"VSWR 1.15:1 over operating band",null,"VSWR 1.15:1 over operating band",null,"VSWR 1.10:1 ",null,"VSWR 1.15:1 over operating band",null,"VSWR,  1.2:1 over operating band",null,"VSWR,  1.15:1 over operating band",null,"VSWR,  1.15:1 over operating band"]
[null,"Horizontally polarized",null,"Horizontally or elliptically polarized ",null,"Horizontally, elliptically or circularly polarized",null,"Input power 1000W average power per panel",null,"500W Average Power Rating PER panel input (2 per panel)",null,"500W average power rating per panel",null,"Input Power 7.5kW 4 bay, 15kW for 8 bay, 22.5kW for 12 bay ",null,"Input Power 7.5kW 4 bay, 15kW for 8 bay, 22.5kW for 12 bay ",null,"Horizontally, elliptically or circularly polarized",null,"Horizontally and elliptically polarized",null,"Horizontally and elliptically polarized"]
[null,"7-16 DIN input ",null,"End fed",null,"Center fed harness",null,"Horizontally polarized",null,"Horizontally, elliptically or circularly polarized",null,"Circularly polarized",null,"Horizontally, elliptically or cirularly polarized",null,"Omnioid Azimuth Pattern",null,"3-1/8” EIA input standard",null,"1 5/8” EIA input standard",null,"4 1/16” EIA input standard"]
[null,"1000 W average power rating",null,"Single sections only 8-bay, 10 bay, and 12 bay options",null,"1-5/8” EIA input standard",null,"Aluminum construction",null,"Aluminum construction",null,"Aluminum construction",null,"Available in 4, 8, and 12 bay at 7.5kW per section",null,"Beam tilt 2 degrees standard",null,"Input power 5kW and 7.5 kW",null,"Input power 2.5 and 5kW",null,"Input Power 20kW 8 bay, 40kW for 16 bay, 60kW for 24 bay "]
[null,"Self-supporting",null,"1-5/8\" input",null,"Input Power 4kW 4 bay, 5kW for 8-12 bay, 8kW for 16 bay ",null,"ABS slot cover enviromental protection",null,"Separate horizontal and vertical inputs on panel",null,"One 7-16 DIN input per panel",null,"Omnioid and Cardioid AZ patterns",null,"Economical alternative to panel antennas",null,"One standard azimuth pattern available",null,"Two standard azimuth patterns available C160 and S230",null,"Two standard azimuth patterns available C160 and S230"]
[null,"Can be side or top mounted on tower",null,"2kW average power rating",null,"Slot covers or radomes enviromental protection",null,null,null,"Two 7-16 DIN input per panel",null,"ABS radome for environmental protection",null,"Slot cover or radome enviromental protection",null,"Low weight and 75% less windload than panels",null,"Two elevation pattern available",null,"Radome enviromental protection",null,"Multiple elevation patterns available"]
[null,"Aluminum construction",null,"ABS slot cover enviromental protection",null,null,null,null,null,"ABS Radome for Environmental Protection",null,null,null,null,null,"Slot cover or radome enviromental protection",null,"Elevation gain 12 (10.7dBd)",null,null,null,"Radome enviromental protection"]
[null,"ABS radome for environmental protection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 degrees nominal beam tilt"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Slot cover or radome enviromental protection"]
[]
[]
[]
[]
[]
[]
[]
[null,"Scroll to the right >>>>>>>>>>"]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}